DSQII

Direct Injection
Samples were measured on a MS system from Thermo Fisher Scientific GmbH (Bremen, Germany) consisting of a DSQII single quadrupole mass spectrometer and a Direct Probe Controller (DPC) injection system using the direct exposure probe (DEP) technique. The sample was placed on the rhenium wire and evaporated using a current slope of 100 mA /s (from 0 to 800 mA). The ion source was set to 200 °C and a scan range was set between 100 and 1050 m/z.

